For 1990-2009 cars

### Removal Procedure

1. Remove the HVAC controller. (Refer to "HVAC Controller" in this service manual)
2. Remove the blower motor switch screws.
3. Remove the blower motor switch.

### Installation Procedure

1. Install the blower motor switch and screws.
2. Install the HVAC controller. (Refer to "HVAC Controller" in this service manual.)

Tighten
Tighten to 2.5 N·m (22 lbs in)