For 1990-2009 cars

## Radio Rear Speaker Replacement Coupe/Sedan

### Removal Procedure

1. Remove the rear window trim finish panel. Refer to Upper Rear Trim Finish Panel Replacement in Interior Trim.
2. Remove the speaker fasteners and pull the speaker away from the panel assembly.
3. Disconnect the speaker wire harness from the speaker.
4. Remove the speaker from the vehicle.

### Installation Procedure

1. Connect the speaker wire harness to the speaker.

Notice: Refer to Fastener Notice in the Preface section.

2. Position the speaker in panel assembly and install the fasteners.

Tighten
Tighten the rear speaker fasteners to 2.5 N·m (22 lb in).

3. Install the rear window trim finish panel. Refer to Upper Rear Trim Finish Panel Replacement in Interior Trim.

## Radio Rear Speaker Replacement Wagon

### Removal Procedure

1. Remove the liftgate inner lower panel assembly. Refer to Liftgate Panel Assembly - Inner Lower in Interior Trim.
2. Remove the speaker fasteners and pull the speaker away from the panel assembly.
3. Disconnect the speaker wire harness from the speaker.
4. Remove the speaker from the vehicle.

### Installation Procedure

1. Connect the speaker wire harness to the speaker.
2. Position the speaker in the panel assembly.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the liftgate speaker fasteners.

Tighten
Tighten the liftgate speaker fasteners to 2.5 N·m (22 lb in).

4. Install the liftgate inner lower panel assembly. Refer to Liftgate Panel Assembly - Inner Lower in Interior Trim.