For 1990-2009 cars

### Removal Procedure

Important: LHD illustrations are shown; RHD illustrations are similar.

1. Remove the left lower trim panel extension by pulling outward at the dual-lock location. Rotate the panel outward to disengage the hinges from the console.
2. Remove the bulb socket from the cigarette lighter by rotating clockwise and pulling it straight out.
3. Disconnect the cigarette lighter electrical connector by spreading the barbs with a screwdriver and then pulling it towards the front of the vehicle.
4. Remove the cigarette lighter assembly by unscrewing the collar behind the bulb holder.

### Installation Procedure

1. Install the socket through the front of the console opening.

Install the bulb holder and the collar. Tighten the collar.

2. Connect the cigarette lighter electrical connector.
3. Install the cigarette lighter bulb through the opening and rotate it counter clockwise.
4. Install the left lower trim panel extensions by inserting the hinges into the console openings. Rotate it towards the I/P retainer and press firmly to engage the dual lock.

'