For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .

Caution: If energy absorber is removed or damaged it must be replaced with a new part. If omitted, the vehicle will not meet federal motor vehicle safety standards (FMVSS), subjecting the retailer to possible civil penalties for making the vehicle inoperative to the FMVSS, and increasing the risk of injury to the vehicle occupants.

2. Remove the energy absorber from the door structure.

### Installation Procedure

1. Remove the tape backing and install to the door structure.
2. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .