For 1990-2009 cars

### Removal Procedure Left Side

1. Reach up from underneath the fascia; then twist and remove the fog lamp bulb socket from the fog lamp.
2. Disconnect the fog lamp bulb from the harness.

### Installation Procedure Left Side

1. Reach up from underneath the fascia to connect the fog lamp bulb to the harness.
2. Twist the fog lamp bulb socket into the fog lamp.

### Removal Procedure Right Side

1. Open hood, twist and remove turn signal bulb from headlamp capsule above fog lamp.
2. Reach down through clearance behind headlamp capsule to twist and remove fog lamp bulb socket.
3. Disconnect fog lamp bulb from harness.

### Installation Procedure Right Side

1. Reach down through the clearance behind the headlamp capsule to connect fog lamp bulb to harness.
2. Twist fog lamp bulb socket into fog lamp.
3. Twist to install turn signal bulb into headlamp capsule.