For 1990-2009 cars

## Back-Up Lamps SC1, SC2 Models Only

For the type of bulb required for replacement, see Replacement Bulbs .

1. Open the decklid. Rotate the bulb socket clockwise and remove it.
2. Depress the tab on the socket assembly with your index finger and rotate it 1/8 of a turn counterclockwise.
3. Remove the bulb from the socket assembly by gently pushing the bulb downward and rotating it 1/8 of a turn counterclockwise. Replace with an appropriate bulb.