For 1990-2009 cars

## Body Side Center Molding Replacement 1st Design

### Removal Procedure

1. Remove the seat belt rocker anchor Torx ® fastener.
2. Slide the seat belt webbing through the slit on the shoulder belt guide.
3. Remove the seat belt retractor cover by pulling on it.
4. Route the seat belt retractor cover down the seat belt webbing.

### Installation Procedure

1. Route the seat belt webbing through the seat belt retractor cover.
2. Install the seat belt retractor cover.
3. Slide the seat belt webbing through the slit on the shoulder belt guide.

Notice: Refer to Fastener Notice in the Preface section.

Caution: Apply Loctite 242® Threadlocker US P/N 12345382 (Canadian P/N 10953489), or equivalent, on all restraint bolts/nuts before installation. Failure to use such threadlocker correctly may result in personal injury.

4. Install the seat belt rocker anchor and Torx® fastener.

Tighten
Tighten the shoulder belt lower attachment fastener to 50 N·m (37 lb ft).