For 1990-2009 cars

Manual Transaxle | 2.5L (2.6 qts.) fluid change
Automatic Transaxle | 4.0L (4.2 qts.) fluid change with pressure filter
Cooling System | 6.6L (7 qts.)
Engine Crankcase (Oil and Filter) | 3.8L (4 qts.)
Fuel Tank | 45.8L (12.1 gal.)
Power Steering - Pump Only - Complete System | 0.40L (14 oz.) 0.80L (28 oz.)
Engine Firing Order | 1-3-4-2
Thermostat Temperature | 88°C (194°F)
Tire Pressure, Sizes | Refer to Tire Placard on the driver's door opening sill below the door striker
Wheel Nut Torque | 140 Nm (103 ft-lbs)

Important: All capacities are approximate. When adding, be sure to fill to the appropriate level of the dipstick, if applicable.