For 1990-2009 cars

### Removal Procedure

1. Drain the cooling system below the engine outlet neck. Refer to Engine Coolant Check and Replacement .
2. Remove the clamp and hose from the radiator inlet neck.
3. Remove the clamp and hose from the engine inlet neck.
4. Remove the hose from the vehicle.

### Installation Procedure

1. Install the hose and clamp on the engine outlet neck. Position the clamp at 1 o'clock.
2. Install the hose and clamp on the radiator inlet neck. Position the clamp at 1 o'clock.
3. Fill the cooling system and perform a leak test. Refer to Engine Coolant Check and Replacement .