For 1990-2009 cars

### Removal Procedure

1. Remove the retainers attaching the wheelhouse panel to the front fascia.
2. Remove the inner plastic fasteners attaching wheelhouse panel to the fender support bracket, motor compartment side panels and inner wheelhouse panel.
3. Remove the plastic fasteners at the outer edge of the wheelhouse panel to the fender attachment location.
4. Remove the wheelhouse panel.

### Installation Procedure

1. Position the wheelhouse panel into location.
2. Install the plastic retainers at the outer edge of panel.
3. Install the inner plastic fasteners.