For 1990-2009 cars

## Steering Column Opening Filler Replacement Left Hand Drive

### Removal Procedure

1. Remove the screws from the data link connector (DLC) and the steering column filler panel.
2. Remove the hood release cable from the lever.
3. Remove the steering column filler panel.

### Installation Procedure

1. Install the hood release cable to the lever.
2. Install the steering column filler panel and the DLC.

Notice: Refer to Fastener Notice in the Preface section.

3. Install and tighten the bolts.

Tighten
Tighten the bolts to 2.2 N·m (20 lb in).

## Steering Column Opening Filler Replacement Right Hand Drive Domestic

### Removal Procedure

1. Remove the screws from the data link connector (DLC) and the steering column filler panel.
2. Lower the steering column filler panel and remove the hood release handle assembly.
3. Remove the steering column filler panel.

### Installation Procedure

1. Install the hood release handle assembly to the steering column filler panel screws.
2. Install the steering column filler panel and the DLC.

Notice: Refer to Fastener Notice in the Preface section.

3. Install and tighten the bolts.

Tighten
Tighten the bolts to 2.2 N·m (20 lb in).