For 1990-2009 cars

### Removal Procedure

1. Remove the retainers and the wheelhouse panel to fascia.
2. Remove the plastic retainers, the rear wheelhouse panel to quarter panel, and the rocker panel cover.
3. Slide the top of the wheelhouse panel out of the quarter panel.
4. Remove the wheelhouse panel.

### Installation Procedure

1. Position the top of the wheelhouse panel to the quarter panel.
2. Install the plastic retainers, the rear wheelhouse panel to quarter panel, and the rocker panel cover.
3. Install the retainers and the wheelhouse panel to fascia.