For 1990-2009 cars

### Removal Procedure

1. Remove the recirc motor electrical connection.
2. Remove the recirc motor mounting screws.
3. Pull the motor straight off of the recirc door shaft.

### Installation Procedure

1. Position the recirc door to the outside air.
2. Align the flats on motor shaft and recirc door shaft.
3. Push the motor straight on the recirc door shaft while rotating back and forth to engage recirc door shaft into recirc motor.
4. Install the mounting screws.

Tighten
Tighten to 1.7 N·m (15 lbs in).

5. Install the electrical connector.