For 1990-2009 cars

### Removal Procedure

Important: Record pre-set radio stations.

1. Disconnect the negative battery cable.
2. Disconnect the positive battery cable.
3. Remove the battery insulating cover.
4. Remove the battery hold down bracket.

Caution: Do not tip the battery over a 45 degree angle or acid could spill causing serious personal injury.

5. Remove the battery.

### Installation Procedure

1. Verify the battery tray is clean.
2. Install the battery.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the battery hold down bracket.

Tighten
Tighten the battery case bracket stud and nut to 9 N·m (80 lb ft).

Notice: Battery life is reduced if a battery insulation cover is not used.

4. Install the battery insulating cover.
5. Verify the battery cable ends are clean and free of corrosion. Clean with a wire brush.
6. Connect the positive battery cable.

Tighten
Tighten the battery terminal bolts to 17 N·m (13 lb ft).

Important: Set the clock and radio pre-set stations.

7. Connect the negative battery cable.

Tighten
Tighten the battery terminal bolts to 17 N·m (13 lb ft).