For 1990-2009 cars

### Removal Procedure

1. Remove the door outer panel. Refer to Front Side Door Outer Panel .

Important: Apply only enough tension so that the sound insulator releases from the door structure.

2. Remove the door sound insulator.

### Installation Procedure

Important: Make sure the attaching points are clean and dry. If the sound insulator has been damaged during removal, it must be replaced.

1. Using the locating holes, position the sound deadener panel to the structure. Make sure the proper alignment is achieved. Improper alignment could cause outer panel misalignment.

Important: If the adhesive on the door sound insulator does not stick, 3M® Trim and Emblem Adhesive P/N 08063, P/N 08061, or equivalent, can be used to adhere the door sound insulator to the door structure.

2. Install the door outer panel. Refer to Front Side Door Outer Panel .