For 1990-2009 cars

## Energy Absorber Pad Replacement - Quarter Inner Panel Coupe Left Side

### Removal Procedure

1. Remove the quarter lower rear trim panel. Refer to Rear Quarter Trim Panel Replacement - Left Side .

Caution: If energy absorber is removed or damaged it must be replaced with a new part. If omitted, the vehicle will not meet federal motor vehicle safety standards (FMVSS), subjecting the retailer to possible civil penalties for making the vehicle inoperative to the FMVSS, and increasing the risk of injury to the vehicle occupants.

2. Remove the quarter inner panel energy absorber. Refer to the following:

• | Quarter lower trim panel (1)

• | Quarter inner panel energy absorber (2)

### Installation Procedure

1. Install the quarter inner panel energy absorber.
2. Install the quarter lower rear trim panel. Refer to Rear Quarter Trim Panel Replacement - Left Side .