For 1990-2009 cars

## Blower Motor Control Processor Replacement LHD Only

### Removal Procedure

1. Disconnect the blower motor electrical connector.
2. Remove the blower motor mounting screws.
3. Remove the blower motor and cover.

### Installation Procedure

1. Install the blower motor and cover.
2. Install the blower motor mounting screws.

Tighten
Tighten the blower motor mounting screws 1.7 N·m (15 lbs in).

3. Install the electrical connector to the blower motor.

## Blower Motor Control Processor Replacement RHD Domestic Only

### Removal Procedure

1. Disconnect the blower motor electrical connector.
2. Remove the blower motor mounting screws.
3. Remove the blower motor assembly.

### Installation Procedure

1. Install the blower motor assembly.
2. Install the blower motor mounting screws.

Tighten
Tighten the blower motor mounting screws 1.7 N·m (15 lbs in).

3. Install the electrical connector to the blower motor.