For 1990-2009 cars

### Removal Procedure

1. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement . The outer panel is removed in the illustration to show the location.
2. Remove the exterior bolt and push up to disengage the guide from the door structure pivot area.

### Installation Procedure

1. Engage the rear door rear window guide tab into the door structure pivot area.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolt into the rear door rear window guide and check for proper operation.

Tighten
Tighten the rear door rear window guide bolts (Sedan/Wagon) to 7.5 N·m (67 lb in).

3. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .