For 1990-2009 cars

### Removal Procedure

Notice: Wagon rear wiper does not have a "Service Up" position. Lifting wiper too far away from glass can damage wiper system.

1. Lift the rear wiper arm away from the glass.
2. Using a small flat blade screwdriver, disengage the wiper arm retaining latch.
3. Remove the wiper blade from the wiper arm.

### Installation Procedure

1. Position the wiper blade to hook onto the wiper arm.
2. Slide the blade assembly into the hook on the wiper arm until it clicks into position.