For 1990-2009 cars

SYSTEM | FUNCTION PROGRAMMED AT FACTORY | FUNCTION RE-PROGRAMMED AT RETAILER
--- | --- | ---
RKE - Door locking audible feedback | Horn chirps once with second lock command within 5 seconds of first. Horn chirps 3 times to signify delayed locking situation. | Horn does not chirp with second lock command or during delayed locking
RKE - Door locking visual feedback | DRLs (daytime running lamps) flash once with lock command or once during delayed locking when all doors and trunk is closed. | The DRLs do not flash with the lock command from key fob
RKE - Door unlocking audible feedback | Horn does not chirp with unlock command. | Horn chirps twice with first unlock command
RKE - Door unlocking visual feedback | DRLs flash twice with unlock command. | DRLs do not flash with unlock command
RKE - Delayed Locking | Lock command is delayed until all doors and trunk are closed. | All doors lock when command is received even if a door(s) or trunk is open
Passive Arming of Saturn Security System | Passive arming is not enabled. | Security system arms automatically when the ignition key is removed and all doors and trunk are closed for 60 seconds or 10 minutes after the ignition key is removed but no doors are opened and closed. Passive arming does not lock doors automatically
Saturn Security System Pre-Alarm | Horn will chirp for 10 seconds before going into full alarm state if a door or the trunk is opened after the system is armed. | Horn will stay silent for 10 seconds before going into full alarm state if a door or the trunk is opened after the system is armed
To change programmable functions refer to the Tech 2 User's Guide.

#### Vehicle Tampered With and Content Theft System Armed - Security Telltale Status/Content Theft Alarm

STATE | DESCRIPTION | SECURITY LED STATUS
--- | --- | ---
Unarmed | Security System disabled. | OFF
IGN ON | Prevents System Arming with IGN ON. | OFF
Program Mode | System Programming Mode. | OFF
Quiet Pre-Alarm | Waiting for Ignition OFF, all doors and trunk to close, then ARM. | ON
ARM | Security System armed. | Flashing
Pre-Alarm | Horn chirps for 10 seconds or BCM chime sounds for 10 seconds. | Flashing
Alarm | Sound horn for 2 minutes, cycle DRL lights for 2 minutes, cycle dome lamp for 2 minutes. | Flashing with horn activation and DRL activation
Tampered | Security System was tampered | Flashing
Warning | Horn will chirp 3 times notifying owner that alarm had been cycled for 2 minute time period |
RE-Tamper | Full alarm - Horn on for 2 minutes and DRL lights on for 2 minutes. | Flashing with horn and DRL lights ON