For 1990-2009 cars

## Front Seat Belt Guide Replacement SC1

### Removal Procedure

1. Slide the seat belt webbing through the slit in the seat belt shoulder guide.
2. Remove the fasteners and the seat belt shoulder guide.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt shoulder guide and the fasteners.

Tighten
Tighten the seat belt shoulder guide fasteners to 5 N·m (44 lb in).

2. Slide the seat belt webbing through the slit in the seat belt shoulder guide.

## Front Seat Belt Guide Replacement SC2

### Removal Procedure

1. Slide the seat belt webbing through the slit on the shoulder belt guide.
2. Remove the headrest.

2.1. | Raise the headrest assembly to the full up position.

2.2. | Push the headrest lever towards the rear of the vehicle.

2.3. | Pull the headrest out of the seatback.

3. Remove the fasteners from underneath the headrest support rods.
4. Slide the seat belt guide down from the headrest support rods.

### Installation Procedure

1. Slide the seat belt guide over the headrest support rods.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fasteners to attach the seat belt guide to the headrest.

Tighten
Tighten the seat belt guide headrest fasteners to 5 N·m (44 lb in).

3. Install the headrest.

3.1. | Align the headrest support rods with the holes in the seatback.

3.2. | Push the headrest lever toward the rear of the vehicle.

3.3. | Push the headrest into the seatback.

4. Slide the seat belt webbing through the slit on the shoulder belt guide.