For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the instrument panel.
3. Remove the screws and the center air outlet duct.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the center air outlet duct and screws.

Tighten
Tighten the center air outlet duct screws to 10 N·m (89 lb in).

Important: Make sure that the right plastic mounting tab is between the knee beam and the mounting bracket.

2. Install the instrument panel.
3. Enable the SIR system. Refer to Enabling the SIR System in SIR.