For 1990-2009 cars

## Rear Side Door Insulator Coupe

### Removal Procedure

1. Remove the rear side door outer panel. Refer to Rear Door Outer Door Panel - Coupe.
2. Remove the rear side door insulator.

### Installation Procedure

1. Install the rear side door insulator to the structure by adhering the upper surface first and then the rearward edge.

Important: Adhere the remainder of the insulator in a clock-wise motion ending at the upper forward corner.

2. If the adhesive or the door sound insulator does not stick, 3M® Trim and Emblem Adhesive P/N 08063, P/N 08061 or equivalent, can be used to adhere the door insulator to the door structure.
3. Install the rear side outer door panel. Refer to Rear Door Outer Door Panel - Coupe.