For 1990-2009 cars

Table 1: | Fuel and Emission System SOHC (L24)/DOHC (LL0)

#### Fuel and Emission System SOHC (L24)/DOHC (LL0)

Measurement | Standard | Service Limit
--- | --- | ---
Metric | English | Metric | English
Air System
Intake Manifold Vacuum, No Load | Idle: 73 kPa | 21 in Hg max. |  |
50 kPa | 15 in Hg min.
Air Inlet Restriction, No Load, Between Air Filter and Throttle Body | 4,000 RPM: 60 kPa | 20 in Hg max. |  |
Crankcase Pressure/Vacuum
At 4,000 RPM, No Load | Positive: 1 kPa | 4 in H2O max. | Positive: 2.5 kPa | 10 in H2O max.
Coolant Temperature 90°C (195°F) | Negative: 3 kPa | 12 in H2O max. | Negative: 3.5 kPa | 14 in H2O max.
Fuel Pump
SOHC (L24)/DOHC (LL0) Dead Head Pressure at 12 volts | 450-650 kPa | 65-94 psi |  |
Pressure Decay | 55 kPa | 8 psi max. |  |
Fuel System SOHC (L24)/DOHC (LL0)
Operating Pressure | 276-370 kPa | 40-55 psi |  |
Pressure Decay in 5 Minutes | 55 kPa | 8 psi max. |  |
Fuel Tank
Capacity | 45.9 L | 12.1 gal |  |

Specification | RPM | Transaxle Gear | Fuel Cut-Off RPM
--- | --- | --- | ---
Idle Speed (RPM) |  |  |
SOHC (L24) Manual (A/C ON/OFF) | 750+/-50 | Neutral | SOHC (L24) | 5750+/-150
SOHC (L24) Automatic | 650+/-50 | Drive | SOHC (L24) | 6000+/-150
SOHC (L24) Automatic, With A/C ON | 775+/-50 | Drive | DOHC (LL0) | 6750+/-150
DOHC (LL0) Manual, With A/C ON | 850+/-50 | Neutral |  |
875+/-50 | Neutral
DOHC (LL0) Automatic, With A/C ON | 750+/-50 | Drive |  |
775+/-50 | Drive
Min. Air Idle Speed SOHC (L24) and DOHC (LL0) | 0 RPM (Stall) to 700 RPM | Neutral |  |
Note: Do not adjust minimum idle speed.