For 1990-2009 cars

Caution: Be careful when you handle a sensing and diagnostic module (SDM). Do not strike or jolt the SDM. Before applying power to the SDM:

• | Remove any dirt, grease, etc. From the mounting surface.

• | Position the SDM horizontally on the mounting surface.

• | Tighten all of the SDM fasteners and SDM bracket fasteners to the specified torque value.

Failure to follow the correct procedures could cause air bag deployment, personal injury, or unnecessary SIR system repairs.

Caution: Proper operation of the supplemental inflatable restraint (SIR) sensing system requires that any repairs to the vehicle structure return the vehicle structure to the original production configuration. Not properly repairing the vehicle structure could cause non-deployment of the air bag in a frontal collision or deployment of the air bag for conditions less severe than intended. Incorrect configuration may result in personal injury.

#### ACCIDENT WITH OR WITHOUT AIR BAG DEPLOYMENT:

After any collision, inspect these components as indicated. If you detect any damage, replace the component. If you find any damage to the mounting hardware, repair or replace the hardware as needed.

• | Steering Column -- Perform the "Checking Steering Column for Accident Damage" procedures in the Repairs and Inspections Required After a Collision section in this service manual.

• | I/P Knee Bolsters -- Inspect the knee bolsters for bending, twisting, buckling, or any type of damage.

• | I/P brackets, braces, etc. -- Inspect for bending, twisting, buckling, or any other type of damage.

• | Seat Belts -- Perform the "Safety Belt Operational Checks" section in the "Body/Repair" service manual.

#### ACCIDENT WITH AIR BAG DEPLOYMENT:

After a collision involving air bag deployment, replace these components. If you detect any damage to the mounting hardware, repair or replace the mounting hardware as needed.

• | Inflatable Restraint I/P (inflator) Module

• | Inflatable Restraint Sensing and Diagnostic Module

• | Inflatable Restraint Steering Wheel (inflator) Module

| After a collision involving air bag deployment, inspect the following components as indicated. Perform these component inspections in addition to the inspection indicated as "Accident With or Without Air Bag Deployment." If you find any damage to the mounting points or mounting hardware, repair the component or replace the hardware as needed.

• | Inflatable Restraint Steering Coil Assembly -- Inspect the coil and the coil wiring pigtail for melting, scorching, or other damage due to excessive heat.

### Removal Installation

Important: In the event deployment has occurred, inspect the coil assembly wire for any signs of scorching, melting or other damage due to excessive heat. If the coil has been damaged, it must be replaced.

1. Disable the SIR system. Refer to Disabling the SIR System .
2. Lift the parking brake lever.
3. Remove the parking brake lever cover screw.
4. Remove the parking brake cover by lifting it straight off the lever.
5. Remove the ashtray from the cup holder by lifting it straight out.
6. Remove the cup holder from the console by pulling upwards starting at the rear edge.
7. Remove the ashtray bulb socket by lifting the tab while sliding the socket upwards. Then pull the socket straight out.
8. Remove the wiring harness from the cup holder.
9. Remove the window switch, if equipped, by sliding the switch forward then lifting at the rear edge. Disconnect the electrical connectors.
10. Remove the rear screw cover by lifting at cut out.
11. Remove the rear console screws.
12. If equipped with center console/arm rest, remove the center console/arm rest from the center console.
13. Remove the left and right lower trim panel extensions by pulling outward at the dual lock locations. Then rotate the panels outward to disengage the hinges from the console.
14. Remove the front console screws.
15. Move the console rearward.
16. Remove the bulb socket from the cigarette lighter by rotating counterclockwise and pulling it straight out.
17. Disconnect the cigarette lighter electrical connector.
18. On automatic transaxle equipped vehicles, tape the shifter button in to clear the shifter opening.
19. Lift the console at the rear. Slide the console rearward and lift straight up to remove.
20. Remove the connector position assurance (CPA) device and disconnect the SDM.
21. Remove the SDM bolts and remove the SDM.

### Installation Procedure

Important: Make sure the SDM is oriented with the arrow facing forward.

1. Install the SDM and bolts to the vehicle.

Tighten
Tighten the bolts to 15 N·m (133.5 lb in).

2. Connect the electrical connector and install the connector position assurance (CPA) device.
3. Place the shifter in neutral.
4. Lower the front of the console over the shifter.

Important: Make sure to place the window/mirror and ashtray light connectors through the openings into position.

5. Lower the rear of the console over the parking brake lever on to the rear mounting pad.
6. Move the console rearward.
7. Connect the cigarette lighter electrical connector.
8. Install the cigarette lighter bulb through the opening and rotate clockwise.

Important: Make sure the upper tabs on the front of the console engage the sheet metal on the lower I/P brace.

9. Move the console forward into position.
10. Install and tighten the front console screws.

Tighten
Tighten the front console screws to 1.2 N·m (11 lb in).

11. Align the rear of the console with the pin on the mounting pad.
12. If equipped with center console/arm rest, position the center console/arm rest to the center console.
13. Install and tighten the screws.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).

14. Install the screw cover.
15. Install the left trim panel extension by inserting the hinges into the console openings. Then rotate until closed and push in at dual lock locations. Wait to install the right trim panel until the fuse is installed during SIR system enabling.
16. Connect the window/mirror switch electrical connectors.
17. Install the window switch by inserting the front edge into the opening. Then push the rear edge down into position.
18. Insert the bulb through the opening until the bulb socket is flush with the cup holder. Push the socket down to engage the lock tab.
19. Install the wiring harness to the cup holder.
20. Install the cup holder by inserting it through the console opening and pushing straight down.
21. Enable the SIR system. Refer to Enabling the SIR System in this service manual.
22. Install the parking brake cover over the lever.

Notice: Do not overtighten screw or it may pull through cover.

23. Install and tighten the screw.

Tighten
Tighten the screw to 1.6 N·m (14 lb in).