For 1990-2009 cars

### Removal Procedure

1. Remove rear door trim panel. Refer to Rear Side Door Trim Panel Replacement . Outer panel is removed in illustration to show location.
2. Remove rear side door stationary window. Refer to Rear Side Door Stationary Window Replacement .
3. Remove rear door window. Refer to Rear Side Door Window Replacement .
4. Remove door frame outer seal.

### Installation Procedure

1. Install rear door outer seal and fully seat into channel and onto door header flange.
2. Install rear door stationary window glass. Refer to Rear Side Door Stationary Window Replacement .
3. Install rear door window. Refer to Rear Side Door Window Replacement .
4. Install rear door applique. Refer to Rear Door Frame Applique Replacement .
5. Reinstall rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .