For 1990-2009 cars

### Removal Procedure

1. Insert Graphic SMPMT88846AA1. Remove the lower I/P closeout panel.
2. Disconnect the clutch start switch from the clutch pedal assembly by sliding it upward.
3. Insert Graphic SMPMT88829AA1. Disconnect the clutch start switch connector from the switch.

### Installation Procedure

1. Insert Graphic SMPMT88829AA1. Connect the clutch start switch electrical connector.
2. Insert the switch tabs into the bracket.
3. Install the lower I/P closeout panel.