For 1990-2009 cars

### Removal Procedure

Notice: Wagon rear wiper does not have a "Service Up" position. Lifting wiper too far away from glass can damage wiper system.

1. Lift the rear wiper arm away from the glass.
2. Remove the existing wiper blade insert by pulling downward at the wiper blade end to disengage the retaining tab. Pull the blade insert out of the wiper blade.

### Installation Procedure

Install the wiper blade insert by sliding it through the wiper blade claws until fully assembled and the wiper arm tab is seated into the wiper blade insert.