For 1990-2009 cars

### Removal Procedure

1. Open the liftgate.
2. Remove the back body outer rear panel by gently pulling rearward on the lower end of the panel, disengaging the 3 clips upward.

### Installation Procedure

1. Position the back body outer rear panel to the vehicle. Use the locating tab to align to the spaceframe.

Notice: To seat panel, apply pressure from top to bottom. Failure to apply pressure from top to bottom can result in damage to roof panel paint.

2. Engage the clips by applying pressure, from top to the bottom of the panel.
3. Close the liftgate.