For 1990-2009 cars

## Battery Tray Replacement A

### Removal Procedure

1. Remove air induction system.
2. Remove the battery. Refer to Battery Replacement .
3. Disconnect the PCM J2 black 28-way connector by moving the locking device toward the fender.
4. Remove the PCM J1 black 80-way connector bolt and disconnect.
5. Remove the PCM attachment bolts and PCM.
6. Remove the battery tray bolts and tray. There is one bolt in the fender well.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the tray and bolts, including the one bolt in the fender well.

Tighten
Tighten the tray-to-fender well bolt to 10 N·m (89 lb in).

Notice: Ground strap must be attached to the PCM attachment bolt. The ground strap is a case ground that provides electromagnetic wave interference (EMI) protection. Correct torque is critical.

2. Install the PCM and attachment bolts.

Tighten
Tighten the PCM attachment bolts to 6 N·m (53 lb in).

3. Connect the PCM J1 black 80-way connector and install the attachment bolt.

Tighten
Tighten the PCM connector-to-PCM bolt to 8 N·m (71 lb in).

4. Connect the PCM J2 black 28-way connector and engage the locking device.
5. Install the battery. Refer to Battery Replacement .
6. Install the air induction system.
7. Set the clock.