For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Air Box Attachment Bolts | 10 N·m | 89 lb in
Air Cleaner Tube-to-Throttle Body Clamp | 2 N·m | 18 lb in
Back-Up Lamp Switch | 23 N·m | 17 lb ft
Battery Hold Down-to-Battery Tray Fasteners | 9 N·m | 80 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Battery Tray-to-Frame Rail Bolts | 10 N·m | 89 lb in
Brake Master Cylinder-to-Brake Booster Nuts | 27 N·m | 20 lb ft
Catalytic Converter-to-Intermediate Exhaust Pipe Nuts | 25 N·m | 18 lb ft
Clutch Fork Ball Stud | 24 N·m | 18 lb ft
Clutch Housing Cover-to-Flywheel Bolts | 25 N·m | 18 lb ft
Clutch Housing-to-Engine Bolts | 140 N·m | 103 lb ft
Clutch Hydraulic Damper Bracket-to-Case Studs | 25 N·m | 18 lb ft
Clutch Pedal Pivot Shaft Attachment Nut | 17 N·m | 13 lb ft
Electronic Ignition Module and Bolts | 8 N·m | 71 lb in
End Cover-to-Case Bolts (In Crisscross Pattern) | 12 N·m | 9 lb ft
Engine Strut Bracket-to-Frame Nuts | 50 N·m | 37 lb ft
Engine-to-Transaxle Stiffening Brace Bolts | 54 N·m | 40 lb ft
Exhaust Manifold Pipe-to-Exhaust Manifold Nuts | 31 N·m | 23 lb ft
Fascia Support-to-Frame Fasteners | 10 N·m | 89 lb in
Flywheel Housing Cover-to-Clutch Housing Bolts | 11 N·m | 8 lb ft
Flywheel-to-Crankshaft Bolts (In Crisscross Pattern) | 80 N·m | 59 lb ft
Frame-to-Body Bolts | 210 N·m | 155 lb ft
Front Console Screw | 2.5 N·m | 22 lb in
Front Exhaust Pipe Hanger Strap Clamp | 60 N·m | 44 lb ft
Front Exhaust Pipe Hanger-to-Powertrain Stiffening Bracket Bolts | 30 N·m | 22 lb ft
Front Lower Control Arm Ball Stud-to-Steering Knuckle Nut | 75 N·m | 55 lb ft
Ground Terminal-to-Top Clutch Housing Studs | 25 N·m | 18 lb ft
I/P Upper Trim Panel Fasteners | 6 N·m | 53 lb ft
Input Shaft Clamp Nut | 150 N·m | 111 lb ft
Intake Manifold Support Bracket-to-Intake Manifold Bolt (LL0) | 30 N·m | 22 lb ft
Intake Manifold Support Bracket-to-Intermediate Shaft Support Bracket Nut (LL0) | 54 N·m | 40 lb ft
Intermediate Shaft Support Bracket-to-Engine Bolts | 54 N·m | 40 lb ft
Output Shaft Clamp Nut | 150 N·m | 111 lb ft
PCM Attachment Bolts | 6 N·m | 53 lb in
Rear Console Screw | 2.5 N·m | 22 lb in
Reverse Shift Lever-to-Clutch Housing Bolts | 14 N·m | 10 lb ft
Shift Cable Pass-Through Grommet Nuts | 6 N·m | 53 lb in
Shift Cable Retainer-to-Floor Pan Bolt | 10 N·m | 89 lb in
Shift Control Housing-to-Case Bolts | 28 N·m | 21 lb ft
Shifter Control Assembly-to-Floor Pan Nuts | 25 N·m | 18 lb ft
Steering Gear-to-Frame Bolt & Nut | 50 N·m | 37 lb ft
Tie Rod-to-Steering Knuckle Nut | 25 + 134° N·m | 19 + 134° lb ft
Transaxle Case-to-Clutch Housing Bolts and Studs (In Sequence) | 28 N·m | 21 lb ft
Transaxle Drain Plug | 30 N·m | 22 lb ft
Transaxle Mount-to-Frame Nut | 50 N·m | 37 lb ft
Transaxle Strut Bracket-to-Case Bolts | 54 N·m | 40 lb ft
Transaxle Strut-to-Midrail Bracket Bolt | 50 N·m | 37 lb ft
Transaxle Strut-to-Transaxle Bracket Bolt | 70 N·m | 52 lb ft
Transaxle-to-Engine Studs | 100 N·m | 74 lb ft
Vehicle Speed Sensor | 26 N·m | 19 lb ft
Wheel Lug Nuts (In Crisscross Pattern) | 140 N·m | 103 lb ft