For 1990-2009 cars

## Liftgate Panel Assembly - Inner Lower Wagon

### Removal Procedure

1. Remove the liftgate window upper molding retainers.
2. Remove the liftgate window upper molding by pulling at the clip locations to disengage the clips.
3. Remove the liftgate side window molding by pulling at the clip locations to disengage the clips.
4. Remove the fasteners from the lower end of the liftgate inner lower panel assembly.
5. Remove the liftgate rubber bumpers.
6. Remove the liftgate inner lower panel by pulling at the clip locations to disengage the clips.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Position the liftgate inner lower panel to the vehicle. Push at the attaching clip locations to engage the clips. Install the fasteners.
2. Install the liftgate rubber bumpers.
3. Position the liftgate side window molding to the vehicle. Push at the attaching clip locations to engage the clips.
4. Position the liftgate window upper molding to the vehicle.
5. Push at the attaching clip locations to engage the clips.
6. Install the retainers.