For 1990-2009 cars

### Removal Procedure

1. Disable the SIR System.
2. Remove console.
3. Remove park brake adjuster nut.
4. Remove park brake cables from equalizer assembly.
5. Pull park brake lever to highest position.
6. Lift equalizer cable over park brake indicator switch and swing forward. Pull cable down and out of park brake lever.

### Installation Procedure

1. Slide equalizer cable into park brake lever. Hand start adjuster nut.
2. Swing equalizer cable rearward and lift over park brake indicator switch.
3. Release and lower park brake lever fully.
4. Install both park brake cables into equalizer.
5. Adjust park brake.
6. Install console.
7. Enable the SIR system.