For 1990-2009 cars

## Hood Release Lever Replacement LHD

### Removal Procedure

1. Using cutting pliers, cut the fasteners off the mounting pins.
2. Remove the hood release lever.

### Installation Procedure

1. Install the hood release lever over the mounting pins.
2. Install the fasteners on the mounting pins.
3. Using a deep well socket, push the fasteners down against the lever.

## Hood Release Lever Replacement RHD Domestic

### Removal Procedure

1. Remove the hood release handle assembly fasteners.
2. Remove the hood release handle assembly.
3. Remove the hood release cable from the lever.

### Installation Procedure

1. Install the hood release cable to the handle assembly.
2. Install the hood release handle assembly to the filler panel.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the hood release handle assembly fasteners.

Tighten
Tighten the hood release lever-to-I/P filler panel fastener to 1.5 N·m (13 lb in).