For 1990-2009 cars

### Removal Procedure

1. Ignition OFF.
2. Use a small flat-bladed screwdriver to pry the switch assembly from the steering wheel.
3. Disconnect the cruise switch harness connector.

### Installation Procedure

1. Connect the switch harness connector. Push in the connector until a click is heard and pull back to confirm a positive engagement.
2. Insert the cruise switch assembly in the steering wheel and gently apply pressure to fasten the switch in the opening.