For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Catalytic Converter-to-Isolator | 25 N·m | 19 lbs ft
Compressor-to-Front-Bracket | 54N·m | 40 lbs ft
Compressor-to-Rear-Bracket | 25 N·m | 19 lbs ft
Converter Flange Nuts | 25 N·m | 19 lbs ft
EGR Pipe-to-Cylinder-Head (LL0) | 25 N·m | 19 lbs ft
EGR Pipe-to-Intake Manifold (LL0) | 10 N·m | 89 lbs in
Exhaust Manifold-to-Head (L24) | 22 N·m | 16 lbs ft
Exhaust Pipe Clamp Nuts | 41 N·m | 30 lbs ft
Exhaust Pipe Clamp-to-Support Bracket | 60 N·m | 44 lbs ft
Exhaust Pipe-to-Manifold | 31 N·m | 23 lbs ft
Fasteners-to-Heat Shield | 10 N·m | 89 lbs in
Forward Exhaust Manifold Stud | 18 N·m | 159 lbs in
Front/Rear Brackets-to-Head/Block | 25 N·m | 19 lbs ft
Intermediate Pipe | 41 N·m | 30 lbs ft
Intermediate Pipe-to-Converter Nuts | 25 N·m | 19 lbs ft
Muffler Hanger Bolt | 12 N·m | 9 lbs ft
Muffler Hanger Bracket | 25 N·m | 19 lbs ft
Muffler Isolator Block-to-Body | 25 N·m | 19 lbs ft
Muffler Mounting Strap Fasteners | 22 N·m | 16 lbs ft
Muffler Strap around Muffler | 22 N·m | 16 lbs ft
Sensor - Oxygen-to-Exhaust Manifold | 45 N·m | 33 lbs ft
Spacer-to-Exhaust Manifold | 10 N·m | 89 lbs in