For 1990-2009 cars

## High Mount Stop Lamp Replacement Coupe

### Removal Procedure

1. Remove the center high-mount stop lamp cover. Pull down by grasping the cover around the edges.
2. Disconnect the electrical harness only if removing the center high-mount stop lamp.
3. If removing the bulbs, twist the sockets out of the stop lamp and remove the bulbs.
4. Remove the center high-mount stop lamp by removing the retainer screws.

### Installation Procedure

1. Install the center high-mount stop lamp with the screws.
2. Connect the electrical harness.
3. Install the cover by placing the tabs in the slots, then firmly press the cover into place.

## High Mount Stop Lamp Replacement Wagon

### Removal Procedure

1. Open the lift gate.
2. Remove the plastic fasteners to the upper garnish molding by pushing the center of the fastener in.
3. Remove the molding.
4. If removing the bulbs, twist the sockets out of the stop lamp and remove the bulbs.
5. Disconnect the electrical harness.
6. Remove the center high mount stop lamp by removing the retainer screws.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the center high mount stop lamp with the screws.

Tighten
Tighten the center high-mount stop lamp (Sedan/Wagon) to 2.5 N·m (19 lb in).

2. Connect the electrical harness.
3. Install the upper garnish molding with the plastic fasteners.
4. Close the lift gate.