For 1990-2009 cars

SYMPTOM | PROCEDURE
--- | ---

• | Front wiper motor does not operate with wiper switch in any position.

• | Front washer pump does not operate.

Chart 1

• | Front wiper motor does not operate with wiper switch in HI position.

• | All other speeds operate normally.

Chart 2

Front wiper operates with wiper switch in HI position only. | Chart 3
Front wiper motor operates with wiper switch in INT position only. | Faulty wiper switch
Front wiper motor does not operate with wiper switch in MIST position. All other speeds operate normally. | Faulty wiper switch
Front wipers stop, then restart after several minutes. | Check for mechanical binding causing motor to overheat
Front washer motor inoperative. | Chart 4
Rear wiper motor inoperative | Chart 5
Rear wiper and washer are inoperative | Chart 6
Rear washer pump inoperative, rear wiper operates normally | Chart 7

Figure 1: |

#### Chart 1

Figure 2: |

#### Chart 2

Figure 3: |

#### Chart 3

Figure 4: |

#### Chart 4

Figure 5: |

#### Chart 5

Figure 6: |

#### Chart 6

Figure 7: |

#### Chart 7