For 1990-2009 cars

### (Option)

If your vehicle has power windows, use the switches on the center console to control each of the windows. The power windows operate only with the ignition in the "RUN" position.

On the four door model, each rear door has a control switch for its own window. In addition, there is a rear window power switch (LOCK) on the center console that turns off electrical power to the rear power window switches on each rear door.

### Automatic (Driver's Power Window)

To lower the driver's window, press the driver's power window switch down lightly. Let it go when the window reaches the desired position.

For automatic operation, press the driver's power window switch all the way down and hold it there momentarily. Then let it go. The window will continue to go down until it is fully open. To stop the automatic function while the window is lowering, lift the switch all the way up and then release it.