For 1990-2009 cars

## Liftgate Side Window Molding Replacement Wagon

### Removal Procedure

1. Remove the liftgate window upper molding retainers.
2. Remove the liftgate window upper moldings by pulling at the clip locations to disengage the clips.
3. Remove the liftgate side window molding by pulling at the clip locations to disengage the clips.

### Installation Procedure

1. Position the liftgate side window molding to the vehicle. Push at the attaching clip locations to engage the clips.
2. Position the liftgate window upper molding to the vehicle. Push at the clip locations to engage the attaching clips.
3. Install the retainers.