For 1990-2009 cars

The lever on the right side of the steering column operates the windshield wipers and washers. Move the wiper lever to the position you want:

(HI): The wipers will run continuously at high speed.
(LO): The wipers will run continuously at low speed.
(INT): Intermittent wiper operation.
(OFF): The wipers are off.
(MIST): The wipers will perform a single wipe when the lever is pushed down momentarily.

Heavy snow or ice can overload your wipers. Clear away snow or ice to prevent an overload. If your windshield wipers are stalled for a few seconds in low speed, an electronic circuit breaker will stop the wiper motor until it cools to protect it from damage. To reset the circuit breaker, move the wiper control switch back to "OFF" and then move to the desired position.

If your windshield wipers are stalled for a few seconds in high speed, the wiper fuse may open. Refer to the section on instrument panel fuse block for fuse replacement information.

### Intermittent Time Delay

In light rain or snow, you might want to use the Intermittent Time Delay (INT) position rather than continuous wiping. Turn the band to choose the delay time. Setting:

• | 1 for a Long Delay,

• | 2 for a Medium Delay, or

• | 3 for a Short Delay.

### Washers

Pull the windshield wiper/washer lever toward you to spray washer fluid on the windshield. The spray will continue until you release the lever. If the wipers are "OFF", the wipers will make three complete wipes and then stop.

### Rear Wiper/Washer (Wagon Models)

The rear wiper switch is a three position rotary switch that is on the same windshield wiper/washer lever on the right side of the steering column. The three positions are:

• | OFF

• | ON

• | WASH

"OFF" and "ON" are fixed positions. The "WASH" position will spray washer fluid onto the back window. The fluid will stop spraying when you release the switch. The wiper will continue to be "ON" until you turn the switch to the "OFF" position.