For 1990-2009 cars

## Front License Plate Bracket Replacement Sedan/Wagon

### Removal Procedure

1. Remove the license plate screws and the license plate.
2. Remove the rivets attaching the license plate bracket to the front fascia.

### Installation Procedure

1. Position the license plate bracket to the front fascia and install the fasteners.

Important: If this is a first time installation, drill 6 mm (0.24 in) hole at dimple on centerline of the lower fascia. Position the bracket to the fascia and install the bottom fastener. Drill two top holes and install the fasteners.

2. Install the license plate to the bracket with screws.

## Front License Plate Bracket Replacement Coupe

### Removal Procedure

1. Remove the license plate screws and the license plate.
2. Remove the rivets attaching the license plate bracket to the front fascia.

### Installation Procedure

1. Position the license plate bracket to the front fascia and install the fasteners.

Important: If this is a first time installation, drill 6 mm (0.24 in) hole at dimple on centerline of the lower fascia. Position the bracket to the fascia and install the bottom rivet. Drill two top holes, using the bracket as a template, and install the rivets.

2. Install license plate to bracket with screws.