For 1990-2009 cars

### Removal Procedure

1. Remove the sunroof glass. Refer to Sunroof Glass Panel Replacement .
2. Remove the seal by pulling from the glass starting at the splice joint.

### Installation Procedure

1. Starting at the rear center of the sunroof glass, install the seal by pushing it onto the edge of the glass panel and gently stretching it.
2. Approximately 102 mm (4 in) prior to completing installation of the seal, cut the seal so there is an extra 3.18 mm (1/8 in) in length.
3. Apply Loctite 410® Black Toughened Instant Adhesive, or equivalent, to the splice joint area where the ends of the seal meet.
4. With approximately 102 mm (4 in) of the seal unattached, push the 2 ends of the seal together in the glue joint.
5. Install the remainder of the seal by pushing the seal onto the edge of the glass panel. The 3.18 mm (1/8 in) of the extra seal material should provide a tight seal at the splice joint.
6. Install the sunroof glass. Refer to Sunroof Glass Panel Replacement .