For 1990-2009 cars

### Removal Procedure

Important: LHD shown; RHD similar

1. Remove the seat from the vehicle. Refer to Front Seat Replacement - Bucket .
2. On the driver's seat, rotate the seat riser knob to the full up position.
3. Remove the recliner handle.
4. On driver's side, remove the seat riser knob cover and fastener.
5. Remove the seat adjuster side covers.
6. On driver's side, install riser knob without screw. Lower the cushion.
7. Disengage the rear J-strip.

• | Seat Cover (1)

• | Cushion Frame (2)

• | Foam Pad (3)

• | Cross Tube (4)

• | Seat Cover J-Strip (5)

8. On the driver's side, raise the seat cushion and remove the riser knob.
9. Remove the bolts at the sides of the seat cushion and remove the seat cushion.
10. Disengage the remaining seat cover J-strips and 2 push fasteners.
11. Remove the seat cushion frame.
12. Pull up on the cover to expose the hog rings (1) and/or separate the Velcro®. Remove the cover.

### Installation Procedure

Important: LHD shown; RHD similar.

1. Transfer the listing wires to the new cover.
2. Install the seat cover over the pad.
3. Install the hog rings (1) around each seat cover listing wire and the seat foam listing wire.
4. Check the fit of the cover and pull on the cover where necessary to remove the wrinkles. Attach the push fasteners.
5. Install the seat cushion assembly to the seat adjuster.

Tighten
Tighten the seat adjuster to 27 N·m (20 lb ft).

6. On the driver's side, install the riser knob without the screw, lower the seat cushion and remove the riser knob.
7. Wrap the seat cushion cover rear flap to the cover up recliner cross tube and engage the seat cushion cover rear J-strip to seat cushion frame.

• | Seat Cover (1)

• | Cushion Frame (2)

• | Foam Pad (3)

• | Cross Tube (4)

• | Seat Cover J-Strip (5)

8. Install the seat adjuster side covers.
9. Install the recliner handle.
10. On the driver's side, install the seat riser knob.
11. Install the seat into the vehicle. Refer to Front Seat Replacement - Bucket