For 1990-2009 cars

### Tools Required

J 42059 Cigar Lighter Removal Tool

### Removal Procedure

1. Remove the 20A LIGHTER fuse (auxiliary fuse) located in the instrument panel fuse block.
2. Obtain the J 42059 .
3. Lift the tether cap from the cigar lighter receptacle.
4. Locate the 2 square holes in the receptacle.
5. Hold the removal tool at a 30 degree angle while inserting it into the receptacle.
6. Position one side of the removal tool in one hole then the other hole.
7. Pull the receptacle straight out.
8. Disconnect the connector.

### Installation Procedure

1. Reconnect the connector.
2. Push the illumination ring and the receptacle (tether cap and receptacle) assembly back into the console.
3. Push the tether cap back into the receptacle.
4. Install the lighter fuse.