For 1990-2009 cars

Important: Do not apply an excessive amount of sealer to an area. An excessive amount of sealer will take longer to dry and could come in contact with body parts or components within the immediate area of the body repair.

After welding any body parts, the areas must be wire brushed and cleaned. When this is done, prime the area with DP90LF Epoxy Primer, mixed with DP401LF Catalyst (or equivalent) before applying the recommended sealer. This will not only waterproof the weld seam, but prevent exhaust gases from entering the passenger compartment. For proper sealing locations, refer to the following illustrations:

Shock Tower

Front Body Hinge Pillar Outer 3/4 Section

Front Body Hinge Pillar Outer 3/4 Section

Front Body Hinge Pillar Outer 3/4 Section

Front Body Hinge Pillar Inner

Rocker Panel Inner

Rear Side Door Ring

Rear Side Door Ring

Rear Side Door Ring

Back Body Pillar - Outer Lower - Wagon

Quarter Rear

Rear Compartment Side

Back Body Pillar - Outer Lower - Wagon

Rear Compartment Side

Quarter Rear

Rear Compartment Side

Quarter Inner Rear

Rear Compartment Rear

Rear Compartment Rear

Windshield Outer

Rear End

Rear Compartment Rear

Rear Compartment Longitudinal

Rear End

Panel - Rocker Inner

B-Pillar