For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Induction Fasteners | 10 N·m | 89 lb in
Battery Case Bracket Stud and Nut | 9 N·m | 80 lb in
Battery Terminal Bolts | 17 N·m | 13 lb ft
Generator Bolts | 32 N·m | 24 lb ft
Generator Positive Terminal | 10 N·m | 89 lb in
Manual Shift Shaft Retaining Nut | 12 N·m | 9 lb ft
PCM Attachment Bolts | 6 N·m | 53 lb in
PCM Connector-to-PCM Bolt | 8 N·m | 71 lb in
Starter Motor-to-Block | 37 N·m | 27 lb ft
Starter Positive Terminal | 10 N·m | 89 lb in
Starter Solenoid Terminal | 5 N·m | 44 lb in
Switch-to-Case Bolts | 14 N·m | 124 lb in
Tray-to-Fender Well Bolt | 10 N·m | 89 lb in
Wheel Nuts | 140 N·m | 103 lb ft