For 1990-2009 cars

## Body Rear Corner Trim Panel Replacement Wagon

### Removal Procedure

1. Remove the rear header trim panel by pulling at the clip locations to disengage the attaching clips.
2. Remove the body rear corner trim panel assembly by pulling at the clip locations to disengage the attaching clips.

### Installation Procedure

1. Position the body rear corner trim panel to the vehicle. Push at the attaching clip locations to engage the clips.
2. Position the rear header trim panel to the vehicle. Push at the attaching clip locations to engage the clips.