For 1990-2009 cars

#### Tools Required

SA91104NE Front Crank Seal Replacer

1. Using a punch or a screwdriver, knock out the oil seal.

1.1. | Clean the seal bore and oil drain back passage.

1.2. | Make sure the oil drain back passage is free of RTV and debris.

2. Install oil seal:

• | Using SA9104E and an arbor press, install a new oil seal. Never tap on the seal or seal installer with a hammer.

• | Apply a thin film of oil to the new seal lip.