For 1990-2009 cars

### Removal Procedure

1. Place a prop under the rear compartment lid that will safely support the lid.
2. Remove the rear compartment lid torque rods. Refer to Rear Compartment Lid Hinge Torque Rod Replacement .
3. Remove the hinge bolts.
4. Remove the rear window trim finish panel. Refer to Upper Rear Trim Finish Panel Replacement in Interior Trim.
5. Remove the hinge to body nuts.
6. Remove the hinge.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the hinge and fasten to the body with the nuts.

Tighten
Tighten the rear compartment hinge to body nuts to 25 N·m (19 lb ft).

2. Slide the hinge arm into the rear compartment lid
3. Install the rear compartment to the hinge bolts.

Tighten
Tighten the rear compartment lid to hinge bolts to 10 N·m (89 lb in).

4. Install the rear compartment lid torque rods. Refer to Rear Compartment Lid Hinge Torque Rod Replacement .
5. Install the compartment lid.
6. Align the rear compartment lid. Refer to Rear Compartment Lid Adjustment .
7. Install the rear window trim finish panel. Refer to Upper Rear Trim Finish Panel Replacement in Interior Trim.